(kicad_symbol_lib
	(version 20251024)
	(generator "kicad_symbol_editor")
	(generator_version "10.0")
	(symbol "Byron771"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(duplicate_pin_numbers_are_jumpers no)
		(property "Reference" "U"
			(at 16.51 12.7 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "Byron771"
			(at 7.874 3.81 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.chbyron.eu/nl-nl/byron-producten/deurbellen-intercoms/bedrade-deuropeningssystemen/byron-00-640-80-771-bedrade-deurbel-00.640.80"
			(at 0 -12.7 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Byron 00.640.80 771 Bedrade deurbel"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "Byron771_0_1"
			(polyline
				(pts
					(xy -1.905 6.985) (xy -1.905 5.715) (xy 2.54 5.715) (xy 2.54 6.985) (xy -1.905 6.985)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 5.08) (xy -0.635 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -0.635 7.62) (xy 0 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 10.795) (xy 0 8.89) (xy 1.905 8.89) (xy 1.905 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 5.08) (xy 0.635 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 1.905) (xy 0 3.81) (xy -1.27 3.81) (xy -1.27 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0.635 7.62) (xy 1.27 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 1.27 5.08) (xy 1.905 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.7 1.905) (xy 12.7 10.795)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "Byron771_1_1"
			(rectangle
				(start -2.54 13.97)
				(end 15.24 -1.27)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type background)
				)
			)
			(text "Ding-Dong"
				(at 7.366 8.636 0)
				(effects
					(font
						(size 1.27 1.27)
					)
				)
			)
			(pin input line
				(at 0 12.7 270)
				(length 0)
				(name "0"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 0 90)
				(length 0)
				(name "3"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 12.7 270)
				(length 0)
				(name "1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 0 90)
				(length 0)
				(name "2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
	(symbol "Byron7770"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(duplicate_pin_numbers_are_jumpers no)
		(property "Reference" "T"
			(at 6.985 15.24 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Value" "Byron7770"
			(at 6.985 5.08 90)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://www.chbyron.eu/nl-nl/byron-producten/deurbellen-intercoms/accessoires/byron-00-640-99-7770-transformator-00.640.99"
			(at -38.1 -10.16 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Power supply, switch-mode power supply unit, 24 V 	PRO INSTA 60W 24V 2.5A 2580230000"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "Byron7770_0_0"
			(rectangle
				(start -0.381 15.621)
				(end -0.381 14.859)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -0.381 15.621)
				(end 0.381 15.621)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -0.381 1.651)
				(end -0.381 0.889)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start -0.381 1.651)
				(end 0.381 1.651)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 15.24)
				(radius 0.635)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 0 1.27)
				(radius 0.635)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0.381 14.859)
				(end -0.381 14.859)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0.381 14.859)
				(end 0.381 15.621)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0.381 0.889)
				(end -0.381 0.889)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 0.381 0.889)
				(end 0.381 1.651)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 3.429 15.621)
				(end 3.429 14.859)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 3.429 15.621)
				(end 4.191 15.621)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 3.429 1.651)
				(end 3.429 0.889)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 3.429 1.651)
				(end 4.191 1.651)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 3.81 15.24)
				(radius 0.635)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(circle
				(center 3.81 1.27)
				(radius 0.635)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 4.191 14.859)
				(end 3.429 14.859)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 4.191 14.859)
				(end 4.191 15.621)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 4.191 0.889)
				(end 3.429 0.889)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(rectangle
				(start 4.191 0.889)
				(end 4.191 1.651)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "8V~"
				(at 1.905 12.7 0)
				(effects
					(font
						(size 1 1)
					)
				)
			)
			(text "1.0A"
				(at 1.905 10.795 0)
				(effects
					(font
						(size 1 1)
					)
				)
			)
			(text "240V~"
				(at 1.905 5.715 0)
				(effects
					(font
						(size 1 1)
					)
				)
			)
			(text "50Hz"
				(at 1.905 3.81 0)
				(effects
					(font
						(size 1 1)
					)
				)
			)
		)
		(symbol "Byron7770_0_1"
			(rectangle
				(start -1.905 16.51)
				(end 5.715 0)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(rectangle
				(start -1.905 13.97)
				(end 5.715 2.54)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
		)
		(symbol "Byron7770_1_1"
			(pin input line
				(at 0 16.51 270)
				(length 0)
				(name "L(+)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 0 90)
				(length 0)
				(name "N(-)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 3.81 16.51 270)
				(length 0)
				(name "N(-)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 3.81 0 90)
				(length 0)
				(name "L(+)"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
