(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "C7-A20X"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 11.43 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Value" "QR-C C7-A20X"
			(at 5.08 1.27 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Footprint" ""
			(at 1.27 13.97 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Datasheet" ""
			(at 12.7 3.81 90)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(effects
				(font
					(size 1.27 1.27)
				)
				(hide yes)
			)
		)
		(symbol "C7-A20X_1_0"
			(rectangle
				(start -6.35 10.16)
				(end 13.97 2.54)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type background)
				)
			)
			(polyline
				(pts
					(xy -3.81 8.255) (xy 0 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 6.985) (xy -3.81 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 5.588) (xy -3.81 4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.81 4.445) (xy 0 4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 6.985) (xy -4.445 6.985) (xy -3.81 5.715) (xy -3.175 6.985)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -3.175 5.715) (xy -4.445 5.715)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -2.54 5.08) (xy 2.54 5.08) (xy 2.54 7.62) (xy -2.54 7.62) (xy -2.54 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -1.27 5.08) (xy 1.27 7.62)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 7.62) (xy 0 10.16)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 0 2.54) (xy 0 5.08)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(text "24V="
				(at -6.35 8.89 0)
				(effects
					(font
						(size 1 1)
					)
					(justify left)
				)
			)
			(text "+"
				(at 0 8.89 0)
				(effects
					(font
						(size 1 1)
					)
					(justify right)
				)
			)
			(text "-"
				(at 0 3.81 0)
				(effects
					(font
						(size 1 1)
					)
					(justify right)
				)
			)
		)
		(symbol "C7-A20X_1_1"
			(polyline
				(pts
					(xy -5.334 6.223) (xy -4.699 6.858)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.334 6.223) (xy -4.953 6.223) (xy -5.334 6.604) (xy -5.334 6.223)
				)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy -5.334 5.461) (xy -4.699 6.096)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy -5.334 5.461) (xy -4.953 5.461) (xy -5.334 5.842) (xy -5.334 5.461)
				)
				(stroke
					(width 0)
					(type solid)
				)
				(fill
					(type outline)
				)
			)
			(polyline
				(pts
					(xy 2.54 6.35) (xy 3.175 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 3.81 6.35) (xy 4.445 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 9.525) (xy 5.08 8.255) (xy 5.715 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 5.08 6.35) (xy 5.715 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 6.35) (xy 6.604 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 6.35) (xy 6.985 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 4.445) (xy 6.985 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 6.35 3.175) (xy 6.35 4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 9.525) (xy 7.62 8.255) (xy 6.985 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 7.62 6.35) (xy 8.255 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 8.89 6.35) (xy 9.525 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 9.525) (xy 10.16 8.255) (xy 10.795 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 10.16 6.35) (xy 10.795 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.43 6.35) (xy 11.684 6.35)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.43 4.445) (xy 12.065 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 11.43 3.175) (xy 11.43 4.445)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(polyline
				(pts
					(xy 12.7 9.525) (xy 12.7 8.255) (xy 12.065 8.255)
				)
				(stroke
					(width 0)
					(type default)
				)
				(fill
					(type none)
				)
			)
			(pin input line
				(at -6.35 6.35 0)
				(length 0)
				(name "Lbl"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 10.16 270)
				(length 0)
				(name "Lbl"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at -5.08 2.54 90)
				(length 0)
				(name "Lbl"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number ""
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 12.7 270)
				(length 2.54)
				(name "A1+"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "A1"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 0 0 90)
				(length 2.54)
				(name "A2-"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "A2"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 5.08 12.7 270)
				(length 2.54)
				(name "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "14"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 6.35 0 90)
				(length 2.54)
				(name "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "11"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 7.62 12.7 270)
				(length 2.54)
				(name "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "12"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 10.16 12.7 270)
				(length 2.54)
				(name "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "24"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 11.43 0 90)
				(length 2.54)
				(name "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "21"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
			(pin input line
				(at 12.7 12.7 270)
				(length 2.54)
				(name "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
				(number "22"
					(effects
						(font
							(size 1.27 1.27)
						)
					)
				)
			)
		)
		(embedded_fonts no)
	)
)
